## 1NC

### 1NC---OFF

#### Text – Private Appropriation of Outer Space except for Space Elevators is Unjust.

#### States ought to position space elevators over lunar heritage sites

#### Space Elevators constitute Appropriation – they impede orbits.

Matignon 19 Louis de Gouyon Matignon 3-3-2019 "LEGAL ASPECTS OF THE SPACE ELEVATOR TRANSPORTATION SYSTEM" <https://www.spacelegalissues.com/space-law-legal-aspects-of-the-space-elevator-transportation-system/> [PhD in space law (co-supervised by both Philippe Delebecque, from Université Paris 1 Panthéon-Sorbonne, France, and Christopher D. Johnson, from Georgetown University || regularly write articles on the website Space Legal Issues so as to popularise space law and public international law]//Elmer

An Earth-based space elevator would consist of a cable with one end attached to the surface near the equator and the other end in space beyond geostationary orbit. An orbit is the curved path through which objects in space move around a planet or a star. The 1967 Treaty’s regime and customary law enshrine the principle of non-appropriation and freedom of access to orbital positions. Space Law and International Telecommunication Laws combined to protect this use against any interference. The majority of space-launched objects are satellites that are launched in Earth’s orbit (a very small part of space objects – scientific objects for space exploration – are launched into outer space beyond terrestrial orbits). It is important to precise that an orbit does not exist: satellites describe orbits by obeying the general laws of universal attraction. Depending on the launching techniques and parameters, the orbital trajectory of a satellite may vary. Sun-synchronous satellites fly over a given location constantly at the same time in local civil time: they are used for remote sensing, meteorology or the study of the atmosphere. Geostationary satellites are placed in a very high orbit; they give an impression of immobility because they remain permanently at the same vertical point of a terrestrial point (they are mainly used for telecommunications and television broadcasting). A geocentric orbit or Earth orbit involves any object orbiting Planet Earth, such as the Moon or artificial satellites. Geocentric (having the Earth as its centre) orbits are organised as follow: 1) Low Earth orbit (LEO): geocentric orbits with altitudes (the height of an object above the average surface of the Earth’s oceans) from 100 to 2 000 kilometres. Satellites in LEO have a small momentary field of view, only able to observe and communicate with a fraction of the Earth at a time, meaning a network or constellation of satellites is required in order to provide continuous coverage. Satellites in lower regions of LEO also suffer from fast orbital decay (in orbital mechanics, decay is a gradual decrease of the distance between two orbiting bodies at their closest approach, the periapsis, over many orbital periods), requiring either periodic reboosting to maintain a stable orbit, or launching replacement satellites when old ones re-enter. 2) Medium Earth orbit (MEO), also known as an intermediate circular orbit: geocentric orbits ranging in altitude from 2 000 kilometres to just below geosynchronous orbit at 35 786 kilometres. The most common use for satellites in this region is for navigation, communication, and geodetic/space environment science. The most common altitude is approximately 20 000 kilometres which yields an orbital period of twelve hours. 3) Geosynchronous orbit (GSO) and geostationary orbit (GEO) are orbits around Earth at an altitude of 35 786 kilometres matching Earth’s sidereal rotation period. All geosynchronous and geostationary orbits have a semi-major axis of 42 164 kilometres. A geostationary orbit stays exactly above the equator, whereas a geosynchronous orbit may swing north and south to cover more of the Earth’s surface. Communications satellites and weather satellites are often placed in geostationary orbits, so that the satellite antennae (located on Earth) that communicate with them do not have to rotate to track them, but can be pointed permanently at the position in the sky where the satellites are located. 4) High Earth orbit: geocentric orbits above the altitude of 35 786 kilometres. The competing forces of gravity, which is stronger at the lower end, and the outward/upward centrifugal force, which is stronger at the upper end, would result in the cable being held up, under tension, and stationary over a single position on Earth. With the tether deployed, climbers could repeatedly climb the tether to space by mechanical means, releasing their cargo to orbit. Climbers could also descend the tether to return cargo to the surface from orbit.

#### Private Companies are pursuing Space Elevators.

Alfano 15 Andrea Alfano 8-18-2015 “All Of These Companies Are Working On A Space Elevator” <https://www.techtimes.com/articles/77612/20150818/companies-working-space-elevator.htm> (Writer at the Tech Times)//Elmer

Space elevators are solid proof that any mundane object sounds way cooler if you stick the word "space" in front of it. But there's much more than coolness at stake when building a space elevator – this technology has the potential to revolutionize space transportation, and the Canadian private space company Thoth Technology that was recently awarded a patent for its space elevator design isn't the only company in the game. One of the other major players is a U.S.-based company called LiftPort Group, founded by space entrepreneur Michael Laine in 2003. Its plan for a space elevator is vastly different from the one for which Thoth received a patent, however. Whereas Thoth's plans entail tethering a 12-mile-high inflatable space elevator to the Earth, LiftPort is shooting for the moon. Originally, LiftPort had planned to build an Earth elevator, too, but it abandoned the idea in 2007 in favor of building a lunar elevator. The basic design for a lunar elevator is an anchor in the moon that is attached to a cable that extends to a space station situated at a very special point. Known as a Lagrange Point, this is the gravitational tipping point between the Earth and the moon, where their gravitational pulls essentially cancel one another out. A robot could then travel up and down the tether, ferrying cargo between the moon and the station. Out farther in space, a counterweight would balance out the system. Both types of space elevator are intended to increase space access, but in very different ways. Thoth's Earth elevator aims to make launches easier by starting off 12 miles above the Earth's surface. LiftPort's space elevator aims to increase access to the moon in particular, because it is much easier to launch a rocket to the Lagrange Point and dock it at a space station than it is to get to the moon directly. There's a third major company based in Japan called Obayashi Corp. whose plans look like a hybrid of Thoth's and LiftPort's. Obayashi is not a space company, however – it's actually a construction company. Like Thoth, Obayashi plans to build an Earth elevator. But its Earth elevator would consist of a cable tethered to the blue planet, a robotic cargo-carrier, a space station, and a counterweight. It essentially looks like LiftPort's plans, but stuck to the Earth instead of to the moon.

#### Yes Space Elevators – NASA confirms.

Snowden 18 Scott Snowden 10-2-2018 "A colossal elevator to space could be going up sooner than you ever imagined" <https://www.nbcnews.com/mach/science/colossal-elevator-space-could-be-going-sooner-you-ever-imagined-ncna915421> (Scott has written about science and technology for 20 years for publications around the world. He covers environmental technology for Forbes.)//Elmer

For more than half a century, rockets have been the only way to go to space. But in the not-too-distant future, we may have another option for sending up people and payloads: a colossal elevator extending from Earth’s surface up to an altitude of 22,000 miles, where geosynchronous satellites orbit. NASA says the basic concept of a space elevator is sound, and researchers around the world are optimistic that one can be built. The Obayashi Corp., a global construction firm based in Tokyo, has said it will build one by 2050, and China wants to build one as soon as 2045. Now an experiment to be conducted soon aboard the International Space Station will help determine the real-world feasibility of a space elevator. “The space elevator is the Holy Grail of space exploration,” says Michio Kaku, a professor of physics at City College of New York and a noted futurist. “Imagine pushing the ‘up’ button of an elevator and taking a ride into the heavens. It could open up space to the average person.”

#### Regardless of completion, Elevators spur investment in Nanotechnology

Liam O’Brien 16. University of Wollongong. 07/2016. “Nanotechnology in Space.” Young Scientists Journal; Canterbury, no. 19, p. 22.

Nanotechnology is at the forefront of scientific development, continuing to astound and innovate. Likewise, the space industry is rapidly increasing in sophistication and competition, with companies such as SpaceX, Blue Origin and Virgin Galactic becoming increasingly prevalent in what could become a new commercial space race. The various space programs over the past 60 years have led to a multitude of beneficial impacts for everyday society. Nanotechnology, through research and development in space has the potential to do the same. Potential applications of nanotechnology in space are numerous, many of them have the potential to capture and inspire generations to come. One of these applications is the space elevator. By using carbon nanotubes, a super light yet strong material, this concept would be an actual physical structure from the surface of the Earth to an altitude of approximately 36 000 km. The tallest building in the world would fit into this elevator over 42 000 times. The counterweight, used to keep the elevator taught, is proposed to be an asteroid. This would need to be at a distance of 100 000 km, a quarter of the distance to the moon. The benefits of such a structure would be enormous. 95% of a space shuttle's weight at take-off is fuel, costing US$ 20 000 per kilogram to send something into space. However, with a space elevator the cost per kilogram can be reduced to as little as US$ 200. Exploration to other planets can begin at the tower, and travel to and from the moon could become as simple as a morning commute to work. Solar sails provide the means to travel large distances and incredible speeds. Much like sails on a boat use wind, the solar sail uses light as a source of propulsion. Ideally these sails would be kilometres in length and only a few micrometres in thickness. This provides us with the ability to travel at speeds previously unheard of. Using carbon nanotubes once again, a solar sail has the capability to travel at 39 756 km/s which is 13% of the speed of light! This sail could reach Pluto in an astonishing 1.7 days, and Alpha Centauri in just 32 years. Space travel to other planets, other stars, could be possible with solar sails. The Planetary Society is funding for a space sail of itself, and has successfully launched one into orbit. NASA has also sent a sail into orbit, allowing it to burn up in the atmosphere after 240 days. Investing time and resources into nanotechnology for space exploration has benefits for society today. Materials such as graphene are being used in modern manufacturing at an increasing rate as the applications become utilised. Carbon nanotubes will change the way we think about materials and their strength. These nanotubes have a tensile strength one hundred times that of steel, yet are only a sixth of the weight. Imagine light weight vehicles using less petrol and energy as well as being just as strong as regular vehicles. With potentials to revolutionize the way we think about space travel, nanotechnology has a bright future. As a new field of science, it has the capability to push the human race to the outer reaches of our galaxy and hopefully one day to other stars. It will inspire generations of explorers and dreamers to challenge themselves and advance the human race into the next era. As Richard Feynman said in his 1959 talk 'There's Plenty of Room at the Bottom' "A field in which little has been done, but in which an enormous amount can be done. There is still plenty more to achieve.

#### Nano tech solves warming

Bhavya Khullar. September 4, 2017. Nanomaterials Could Combat Climate Change and Reduce Pollution. https://www.scientificamerican.com/article/nanomaterials-could-combat-climate-change-and-reduce-pollution/

The list of environmental problems that the world faces may be huge, but some strategies for solving them are remarkably small. First explored for applications in microscopy and computing, nanomaterials—materials made up of units that are each thousands of times smaller than the thickness of a human hair—are emerging as useful for tackling threats to our planet’s well-being. Scientists across the globe are developing nanomaterials that can efficiently use carbon dioxide from the air, capture toxic pollutants from water and degrade solid waste into useful products. “Nanomaterials could help us mitigate pollution. They are efficient catalysts and mostly recyclable. Now, they have to become economical for commercialization and better to replace present-day technologies completely,” says [Arun Chattopadhyay](http://www.iitg.ac.in/arun/), a member of the chemistry faculty at the Center for Nanotechnology, Indian Institute of Technology Guwahati. To help slow the climate-changing rise in atmospheric CO2levels, researchers have developed nanoCO2 harvesters that can suck atmospheric carbon dioxide and deploy it for industrial purposes. “Nanomaterials can convert carbon dioxide into useful products like alcohol. The materials could be simple chemical catalysts or photochemical in nature that work in the presence of sunlight,” says Chattopadhyay, who has been working with nanomaterials to tackle environmental pollutants for more than a decade. Many research groups are working to address a problem that, if solved, could be a holy grail in combating climate change: how to pull CO2 out of the atmosphere and convert it into useful products. Chattopadhyay isn’t alone. Many research groups are working to address a problem that, if solved, could be a holy grail in combating climate change: how to pull CO2 out of the atmosphere and convert it into useful products. Nanoparticles offer a promising approach to this because they have a large surface-area-to-volume ratio for interacting with CO2 and properties that allow them to facilitate the conversion of CO2into other things. The challenge is to make them economically viable. Researchers have tried everything from metallic to carbon-based nanoparticles to reduce the cost, but so far they haven’t become efficient enough for industrial-scale application. One of the most recent points of progress in this area is work by scientists at the CSIR-Indian Institute of Petroleum and the Lille University of Science and Technology in France. The researchers developed a nanoCO2 harvester that uses water and sunlight to convert atmospheric CO2 into methanol, which can be employed as an engine fuel, a solvent, an antifreeze agent and a diluent of ethanol. Made by wrapping a layer of modified graphene oxide around spheres of copper zinc oxide and magnetite, the material looks like a miniature golf ball, captures CO2 more efficiently than conventional catalysts and can be readily reused, according to Suman Jain, senior scientist of the Indian Institute of Petroleum, Dehradun in India, who developed the nanoCO2harvester. Jain says that the nanoCO2 harvester has a large molecular surface area and captures more CO2 than a conventional catalyst with similar surface area would, which makes the conversion more efficient. But due to their small size, the nanoparticles have a tendency to clump up, making them inactive with prolonged use. Jain adds that synthesizing useful nanoparticle-based materials is also challenging because it’s hard to make the particles a consistent size. Chattopadhyay says the efficiency of such materials can be improved further, providing hope for useful application in the future. CLEANSING WATER Most toxic dyes used in textile and leather industries can be captured with nanoparticles. “Water pollutants such as dyes from human-created waste like those from tanneries could get to natural sources of water like deep tube wells or groundwater if wastewater from these industries is left untreated,” says Chattopadhyay. “This problem is rather difficult to solve.” An international group of researchers led by professor Elzbieta Megiel of the University of Warsaw in Poland reports that nanomaterials have been widely studied for removing heavy metals and dyes from wastewater. According to the research team, adsorption processes using materials containing magnetic nanoparticles are highly effective and can be easily performed because such nanoparticles have a large number of sites on their surface that can capture pollutants and don’t readily degrade in water. Chattopadhyay adds that appropriately designed magnetic nanomaterials can be used to separate pollutants such as arsenic, lead, chromium and mercury from water. However, the nanotech-based approach has to be more efficient than conventional water purification technology to make it worthwhile. In addition to removing dyes and metals, nanomaterials can also be used to clean up oil spills. Researchers led by Pulickel Ajayan at Rice University in Houston, Texas, have developed a reusable nanosponge that can remove oil from contaminated seawater.

#### Warming causes Extinction

Kareiva 18, Peter, and Valerie Carranza. "Existential risk due to ecosystem collapse: Nature strikes back." Futures 102 (2018): 39-50. (Ph.D. in ecology and applied mathematics from Cornell University, director of the Institute of the Environment and Sustainability at UCLA, Pritzker Distinguished Professor in Environment & Sustainability at UCLA)//Re-cut by Elmer

In summary, six of the nine proposed planetary boundaries (phosphorous, nitrogen, biodiversity, land use, atmospheric aerosol loading, and chemical pollution) are unlikely to be associated with existential risks. They all correspond to a degraded environment, but in our assessment do not represent existential risks. However, the three remaining boundaries (**climate change**, global **freshwater** cycle, **and** ocean **acidification**) do **pose existential risks**. This is **because of** intrinsic **positive feedback loops**, substantial lag times between system change and experiencing the consequences of that change, and the fact these different boundaries interact with one another in ways that yield surprises. In addition, climate, freshwater, and ocean acidification are all **directly connected to** the provision of **food and water**, and **shortages** of food and water can **create conflict** and social unrest. Climate change has a long history of disrupting civilizations and sometimes precipitating the collapse of cultures or mass emigrations (McMichael, 2017). For example, the 12th century drought in the North American Southwest is held responsible for the collapse of the Anasazi pueblo culture. More recently, the infamous potato famine of 1846–1849 and the large migration of Irish to the U.S. can be traced to a combination of factors, one of which was climate. Specifically, 1846 was an unusually warm and moist year in Ireland, providing the climatic conditions favorable to the fungus that caused the potato blight. As is so often the case, poor government had a role as well—as the British government forbade the import of grains from outside Britain (imports that could have helped to redress the ravaged potato yields). Climate change intersects with freshwater resources because it is expected to exacerbate drought and water scarcity, as well as flooding. Climate change can even impair water quality because it is associated with heavy rains that overwhelm sewage treatment facilities, or because it results in higher concentrations of pollutants in groundwater as a result of enhanced evaporation and reduced groundwater recharge. **Ample clean water** is not a luxury—it **is essential for human survival**. Consequently, cities, regions and nations that lack clean freshwater are vulnerable to social disruption and disease. Finally, ocean acidification is linked to climate change because it is driven by CO2 emissions just as global warming is. With close to 20% of the world’s protein coming from oceans (FAO, 2016), the potential for severe impacts due to acidification is obvious. Less obvious, but perhaps more insidious, is the interaction between climate change and the loss of oyster and coral reefs due to acidification. Acidification is known to interfere with oyster reef building and coral reefs. Climate change also increases storm frequency and severity. Coral reefs and oyster reefs provide protection from storm surge because they reduce wave energy (Spalding et al., 2014). If these reefs are lost due to acidification at the same time as storms become more severe and sea level rises, coastal communities will be exposed to unprecedented storm surge—and may be ravaged by recurrent storms. A key feature of the risk associated with climate change is that mean annual temperature and mean annual rainfall are not the variables of interest. Rather it is extreme episodic events that place nations and entire regions of the world at risk. These extreme events are by definition “rare” (once every hundred years), and changes in their likelihood are challenging to detect because of their rarity, but are exactly the manifestations of climate change that we must get better at anticipating (Diffenbaugh et al., 2017). Society will have a hard time responding to shorter intervals between rare extreme events because in the lifespan of an individual human, a person might experience as few as two or three extreme events. How likely is it that you would notice a change in the interval between events that are separated by decades, especially given that the interval is not regular but varies stochastically? A concrete example of this dilemma can be found in the past and expected future changes in storm-related flooding of New York City. The highly disruptive flooding of New York City associated with Hurricane Sandy represented a flood height that occurred once every 500 years in the 18th century, and that occurs now once every 25 years, but is expected to occur once every 5 years by 2050 (Garner et al., 2017). This change in frequency of extreme floods has profound implications for the measures New York City should take to protect its infrastructure and its population, yet because of the stochastic nature of such events, this shift in flood frequency is an elevated risk that will go unnoticed by most people. 4. The combination of positive feedback loops and societal inertia is fertile ground for global environmental catastrophes **Humans** are remarkably ingenious, and **have adapted** to crises **throughout** their **history**. Our doom has been repeatedly predicted, only to be averted by innovation (Ridley, 2011). **However**, the many **stories** **of** human ingenuity **successfully** **addressing** **existential risks** such as global famine or extreme air pollution **represent** environmental c**hallenges that are** largely **linear**, have immediate consequences, **and operate without positive feedbacks**. For example, the fact that food is in short supply does not increase the rate at which humans consume food—thereby increasing the shortage. Similarly, massive air pollution episodes such as the London fog of 1952 that killed 12,000 people did not make future air pollution events more likely. In fact it was just the opposite—the London fog sent such a clear message that Britain quickly enacted pollution control measures (Stradling, 2016). Food shortages, air pollution, water pollution, etc. send immediate signals to society of harm, which then trigger a negative feedback of society seeking to reduce the harm. In contrast, today’s great environmental crisis of climate change may cause some harm but there are generally long time delays between rising CO2 concentrations and damage to humans. The consequence of these delays are an absence of urgency; thus although 70% of Americans believe global warming is happening, only 40% think it will harm them (http://climatecommunication.yale.edu/visualizations-data/ycom-us-2016/). Secondly, unlike past environmental challenges, **the Earth’s climate system is rife with positive feedback loops**. In particular, as CO2 increases and the climate warms, that **very warming can cause more CO2 release** which further increases global warming, and then more CO2, and so on. Table 2 summarizes the best documented positive feedback loops for the Earth’s climate system. These feedbacks can be neatly categorized into carbon cycle, biogeochemical, biogeophysical, cloud, ice-albedo, and water vapor feedbacks. As important as it is to understand these feedbacks individually, it is even more essential to study the interactive nature of these feedbacks. Modeling studies show that when interactions among feedback loops are included, uncertainty increases dramatically and there is a heightened potential for perturbations to be magnified (e.g., Cox, Betts, Jones, Spall, & Totterdell, 2000; Hajima, Tachiiri, Ito, & Kawamiya, 2014; Knutti & Rugenstein, 2015; Rosenfeld, Sherwood, Wood, & Donner, 2014). This produces a wide range of future scenarios. Positive feedbacks in the carbon cycle involves the enhancement of future carbon contributions to the atmosphere due to some initial increase in atmospheric CO2. This happens because as CO2 accumulates, it reduces the efficiency in which oceans and terrestrial ecosystems sequester carbon, which in return feeds back to exacerbate climate change (Friedlingstein et al., 2001). Warming can also increase the rate at which organic matter decays and carbon is released into the atmosphere, thereby causing more warming (Melillo et al., 2017). Increases in food shortages and lack of water is also of major concern when biogeophysical feedback mechanisms perpetuate drought conditions. The underlying mechanism here is that losses in vegetation increases the surface albedo, which suppresses rainfall, and thus enhances future vegetation loss and more suppression of rainfall—thereby initiating or prolonging a drought (Chamey, Stone, & Quirk, 1975). To top it off, overgrazing depletes the soil, leading to augmented vegetation loss (Anderies, Janssen, & Walker, 2002). Climate change often also increases the risk of forest fires, as a result of higher temperatures and persistent drought conditions. The expectation is that **forest fires will become more frequent** and severe with climate warming and drought (Scholze, Knorr, Arnell, & Prentice, 2006), a trend for which we have already seen evidence (Allen et al., 2010). Tragically, the increased severity and risk of Southern California wildfires recently predicted by climate scientists (Jin et al., 2015), was realized in December 2017, with the largest fire in the history of California (the “Thomas fire” that burned 282,000 acres, https://www.vox.com/2017/12/27/16822180/thomas-fire-california-largest-wildfire). This **catastrophic fire** embodies the sorts of positive feedbacks and interacting factors that **could catch humanity off-guard and produce a** true **apocalyptic event.** Record-breaking rains produced an extraordinary flush of new vegetation, that then dried out as record heat waves and dry conditions took hold, coupled with stronger than normal winds, and ignition. Of course the record-fire released CO2 into the atmosphere, thereby contributing to future warming. Out of all types of feedbacks, water vapor and the ice-albedo feedbacks are the most clearly understood mechanisms. Losses in reflective snow and ice cover drive up surface temperatures, leading to even more melting of snow and ice cover—this is known as the ice-albedo feedback (Curry, Schramm, & Ebert, 1995). As snow and ice continue to melt at a more rapid pace, millions of people may be displaced by flooding risks as a consequence of sea level rise near coastal communities (Biermann & Boas, 2010; Myers, 2002; Nicholls et al., 2011). The water vapor feedback operates when warmer atmospheric conditions strengthen the saturation vapor pressure, which creates a warming effect given water vapor’s strong greenhouse gas properties (Manabe & Wetherald, 1967). Global warming tends to increase cloud formation because warmer temperatures lead to more evaporation of water into the atmosphere, and warmer temperature also allows the atmosphere to hold more water. The key question is whether this increase in clouds associated with global warming will result in a positive feedback loop (more warming) or a negative feedback loop (less warming). For decades, scientists have sought to answer this question and understand the net role clouds play in future climate projections (Schneider et al., 2017). Clouds are complex because they both have a cooling (reflecting incoming solar radiation) and warming (absorbing incoming solar radiation) effect (Lashof, DeAngelo, Saleska, & Harte, 1997). The type of cloud, altitude, and optical properties combine to determine how these countervailing effects balance out. Although still under debate, it appears that in most circumstances the cloud feedback is likely positive (Boucher et al., 2013). For example, models and observations show that increasing greenhouse gas concentrations reduces the low-level cloud fraction in the Northeast Pacific at decadal time scales. This then has a positive feedback effect and enhances climate warming since less solar radiation is reflected by the atmosphere (Clement, Burgman, & Norris, 2009). The key lesson from the long list of potentially positive feedbacks and their interactions is that **runaway climate change,** and runaway perturbations have to be taken as a serious possibility. Table 2 is just a snapshot of the type of feedbacks that have been identified (see Supplementary material for a more thorough explanation of positive feedback loops). However, this list is not exhaustive and the possibility of undiscovered positive feedbacks **portends** even greater **existential risks**. The many environmental crises humankind has previously averted (famine, ozone depletion, London fog, water pollution, etc.) were averted because of political will based on solid scientific understanding. We cannot count on complete scientific understanding when it comes to positive feedback loops and climate change.

#### Space Elevators solve Space Debris – reduces Rocket Launches

Forgan 19, Duncan H. Solving Fermi's Paradox. Vol. 10. Cambridge University Press, 2019. (Associate Lecturer at the Centre for Exoplanet Science at the University of St Andrews, Scotland, founding member of the UK Search for Extra-terrestrial Intelligence (SETI) research network and leads UK research efforts into the search)//Elmer

All objects in HEO reside beyond the geostationary orbit (GEO). The orbital period at GEO (w'hich is aligned with the Earth's equator) is equal to the Earth’s rotational period. As a result, from a ground observer’s perspective the satellite resides at a fixed point in the sky, with clear advantages for uses such as global communication. Activities at HEO are considerably less than at LEO and MEO. Earth's orbital environment does contain a natural component - the meteoroids. These pose little to no threat to space operations - the true threat is self-derived. The current limitations of spacefaring technology ensure that every launch is accompanied by substantial amounts of space debris. This debris ranges in size from dust grains to paint flecks to large derelict spacecraft and satellites. According to NASA’s Orbital Debris Program Office, some 21.000 objects greater than 10 cm in size are currently being tracked in LEO. with the population below 10 cm substantially higher. Most debris produced at launch tends to be deposited with no supplemental velocity - hence these objects tend to follow the initial launch trajectory, which often orbits with high eccentricity and inclination. However, these orbits do intersect with the orbits of Earth’s artificial satellite population, resulting in impacts w'hich tend to produce further debris. The vast majority of the low-size debris population is so-called fragmentation debris. This is produced during spacecraft deterioration, and in the most abun- dance during spacecraft break-up and impacts. The first satellite-satellite collision occurred in 1961. resulting in a 400% increase in fragmentation debris (Johnson et al.. 2008). Most notably, a substantial source of fragmentation debris was the deliberate destruction of the Fengyun 1C satellite by the People’s Republic of China, which created approximately 2.000 debris fragments. As with collisions of ‘natural debris’, debris-debris collisions tend to result in an increased count of debris fragments. Since the late 1970s, it has been understood that man-made debris could pose an existential risk to space operations. Kessler and Cour-Palais (1978) worked from the then-population of satellites to extrapolate the debris production rate over the next 30 years. Impact rates on spacecraft at any location. /, can be calculated if one knows the local density of debris p, the mean relative velocity vrei\* and the cross-sectional area ct: [[EQUATION 13.5 OMITTED]] Each impact increases p without substantially altering vrel or o. We should there- fore expect the impact rate (and hence the density of objects) to continue growing at an exponential rate: [[EQUATION 13.6 OMITTED]] Kessler and Cour-Palais (1978) predicted that by the year 2000, p would have increased beyond the critical value for generating a collisional cascade. As new collisions occur, these begin to increase ^jjp, which in turn increases resulting in a rapid positive feedback, with p and I reaching such large values that LEO is rendered completely unnavigable. This has not come to pass - LEO remains navigable, partially due to a slight overprediction of debris produced by individual launches. The spectre of a collisional cascade (often referred to as Kessler syndrome) still looms over human space exploration, as debris counts continue to rise. Without a corresponding dedicated effort to reduce these counts, either through mitigating strategies to reduce the production of debris during launches, or through removal of debris fragments from LEO. we cannot guarantee the protection of the current flotilla of satellites, leaving our highly satellite-dependent society at deep risk. What strategies can be deployed to remove space debris? Almost all debris removal techniques rely on using the Earth’s atmosphere as a waste disposal sys- tem. Most debris is sufficiently small that atmospheric entry would result in its complete destruction, with no appreciable polluting effects. Atmospheric entry requires the debris fragments to be decelerated so that their orbits begin to intersect with lower atmospheric altitudes. Once a critical altitude is reached, atmospheric drag is sufficiently strong that the debris undergoes runaway deceleration and ultimately destruction. There are multiple proposed techniques for decelerating debris. Some mechani- cal methods include capturing the debris using either a net or harpoon, and applying a modest level of reverse thrust. These are most effective for larger fragments, and especially intact satellites (Forshaw et al., 2015). Attaching sails to the debris is also a possibility if the orbit is sufficiently low for weak atmospheric drag. The Japanese space agency JAXA’s Kounotori Integrated Tether Experiment (KITE) will trail a long conductive cable. As a current is passed through the cable, and the cable traverses the Earth’s magnetic field, the cable experiences a magnetic drag force that will de-orbit the spacecraft. Orbiting and ground-based lasers can decelerate the debris through a variety of means. For small debris fragments, the radiation pressure produced by the laser can provide drag. A more powerful laser can act on larger debris fragments through ablation. As the laser ablates the debris, the resulting recoil generated by the escaping material produces drag and encourages de-orbit. A more lateral solution is to ensure that launches and general space-based activity no longer generate debris. These approaches advocate lower-energy launch mechanisms that do not rely on powerful combustion. The most famous is the space elevator (see Aravind. 2007). Originally conceived by Tsiolkovsky, the ele- vator consists of an extremely durable cable extended from a point near the Earth’s equator, up to an anchor point located at GEO (most conceptions of the anchor point envision an asteroid parked in GEO). ‘Climber’ cars can then be attached to the cable and lifted to LEO, MEO and even GEO by a variety of propulsion methods. Most notably, the cars can be driven to GEO without the need for chemical rockets or nuclear explosions - indeed, a great deal of energy can be saved by having coupled cars, one ascending and one descending. Space elevators would solve a great number of problems relating to entering (and leaving) Earth orbit, substantially reducing the cost of delivering payload out of the Earth's atmosphere. The technical challenges involved in deploying a cable tens of thousands of kilometres long are enormous, not to mention the material science required to produce a cable of sufficient tensile strength and flexibility in the first place. The gravitational force (and centrifugal force) felt by the cable will vary significantly along its length. As cars climb the cable, the Coriolis force will move the car (and cable) horizontally also, providing further strain on the cable material. The relatively slow traversal of the biologically hazardous Van Allen Belt on the route to GEO is also a potential concern for crewed space travel. Whatever the means, a spacefaring civilisation (or at least, a civilisation that utilises its local orbital environment as we do) must develop a non-polluting solution to space travel, whether that is via the construction of a space elevator, a maglev launch loop, rail gun, or some other form of non-rocket acceleration. If it cannot perform pollution-free spacecraft launches (or fully clean up its pollution), then it will eventually succumb to Kessler syndrome, with potentially drastic consequences for future space use, with likely civilisation-ending effects (Solution C.13).

### 1NC---OFF

#### Interpretation – At all TOC bid tournaments, Debaters must open source all constructive positions within 30 minutes of each debate on the NDCA 2021-2022 LD wiki.

Graphical user interface

Description automatically generated with medium confidence

#### Violation: they haven’t disclosed their peninsula aff rounds – that is specifically important since they broke a new aff but we cant access it

#### 1] Research- debaters won’t make it an entire topic with the same case unless they update it and frontline nuanced positions—disclosure allows for more specific research and goes into more depth about the topic 2] Accessibility – disclosure is key to smaller school debaters alleviating big school prep outs – they’re able to scout but small school debaters don’t have the teams to figure out the affs being read. Disclosure is inevitable – the question is whether it happens on a mutually accessible forum. 3] Evidence – disclosure is the only way to verify before round cards aren’t miscut – otherwise you could have unethically misrepresented authors

#### Fairness is a voter cause every arg assumes its being evaluated fairly and education is the only reasons school fund debate

#### Drop the debater to deter future abuse and set good norms

#### Competing Interpretations – a] Race to the bottom of the worst possible theory norms – B] Reasonability bad cause it invites arbitrary judge intervention

#### No Rvis

#### A - Forcing the 1NC to go all in on the shell kills substance education and neg strat which outweighs on timeframe, B - discourages checking real abuse which outweighs on norm-setting and constituvisim C - Encourages baiting – outweighs because if the shell is frivolous, they can beat it quickly D – its illogical for you to win for proving you were fair – outweighs since logic is a litmus test for other arguments

#### Reject 1AR theory- A] 7-6 time skew means it’s endlessly aff biased B] I don’t have a 3nr which allows for endless extrapolation C] 1AR theory is skewed to the aff because they have a 2ar judge psychology warrant.

#### Infinite abuse claims are wrong- A] Spikes solve-you can just preempt paradigms in the 1AC B] Functional limits- 1nc is only 7 minutes long

#### 1NC theory first - 1] Abuse was self-inflicted- They started the chain of abuse and forced me down this strategy 2] Norming- We have more speeches to norm over whether it’s a good idea since the shell was read earlier.

#### Neg abuse outweighs Aff abuse – 1] Infinite prep time before round to frontline 2] 2AR judge psychology and 1st and last speech 3] Infinite perms and uplayering in the 1AR.

#### Reasonability on 1AR shells – 1AR theory is very aff-biased because the 2AR gets to line-by-line every 2NR standard with new answers that never get responded to– reasonability checks 2AR sandbagging by preventing really abusive 1NCs while still giving the 2N a chance.

#### DTA on 1AR shells - They can blow up a blippy 20 second shell to 3 min of the 2AR while I have to split my time and can’t preempt 2AR spin which necessitates judge intervention and means 1AR theory is irresolvable so you shouldn’t stake the round on it.

#### RVIs on 1AR theory – 1AR being able to spend 20 seconds on a shell and still win forces the 2N to allocate at least 2:30 on the shell which means RVIs check back time skew – ows on quantifiability

#### No new 1ar theory paradigm issues- A] the 1NC has already occurred with current paradigm issues in mind so new 1ar paradigms moot any theoretical offense B] introducing them in the aff allows for them to be more rigorously tested which o/w’s on time frame since we can set higher quality norms.

#### Evaluate 1AR Voting issues after the 2NR- It’s key to reciprocity since it means we both get 1 speech each instead of them getting a 2ar to blow them up